;------------------------------------------------------------------
; 
;   emVideo.inf -- This file contains installation information for
;                  eMPIA USB 2.0 Video Devices: EM27xx and EM28xx.
;
;   This installation is for Windows 2000 and XP.
;
;   Copyright (C) LWS 2004-2005 
;                            
;------------------------------------------------------------------

; The current settings are for installation to IMAGE class.
;
; To install to MEDIA class -- 
; 1. uncomment   the Class and ClassGUID lines for MEDIA class, and
; 2. comment out the Class and ClassGUID lines for IMAGE class.
;
[Version]
signature   = "$CHICAGO$"
;Class      = Media                                     ;;; for MEDIA class
;ClassGUID  = {4d36e96c-e325-11ce-bfc1-08002be10318}    ;;; for MEDIA class
Class       = Image                                     ;;; for IMAGE class
ClassGUID   = {6bdd1fc6-810f-11d0-bec7-08002be2092f}    ;;; for IMAGE class
Provider    = %Vendor%
CatalogFile = etWHQL.cat
DriverVer   = 10/20/2005, 2.5.1020.1114

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames]
1 = %DiskLabel%,etDevice.sys,,

[SourceDisksFiles]
etProp.ax      = 1
etVFW.dll      = 1
emYUV.dll      = 1
etUSD.dll      = 1
etScan.sys     = 1
etFilter.sys   = 1
etDevice.sys   = 1
etTwain.ds     = 1
etTwnXP.ds     = 1
etMon.exe      = 1
etRun.exe      = 1

[DestinationDirs]
DefaultDestDir = 11
CAP.CopyDLL    = 11
CAP.CopySTI    = 11
CAP.CopyWIA    = 10
CAP.CopyEXE    = 10
CAP.CopySYS    = 10,system32\drivers
CAP.CopyTwain  = 10,twain_32\USB2800
CAP.CopyTwnXP  = 10,twain_32\USB2800

[Manufacturer]
%Vendor% = Models, NT, NT.5.1

[Models]
%USB2750.DeviceDesc% = USB2750,USB\VID_1578&PID_800C



[Models.NT]
%USB2750.DeviceDesc% = USB2750,USB\VID_1578&PID_800C


[Models.NT.5.1]
%USB2750.DeviceDesc% = USB2750,USB\VID_1578&PID_800C



;---------------------  U S B 2 7 1 0  --------------------

[USB2710]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2710.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2710.XP]
Include       = ks.inf, kscaptur.inf, ksfilter.inf, sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT, STI.WIAVideo.Registration
AddReg        = CAP.AddReg, WIAUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyWIA, CAP.CopyEXE, CAP.CopyTwnXP
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 3
DeviceSubType = 1
Capabilities  = 0x11
Events        = STI.Events
DeviceData    = WIA.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"


;------------ H W ------------

[USB2710.HW]
AddReg = InstFilter2710

[InstFilter2710]
HKR,,UpperFilters,0,"etScan.sys"
HKR,,LowerFilters,0,"etFilter.sys"


[USB2710.NT.HW]
AddReg = InstFilter2710NT

[USB2710.XP.HW]
AddReg = InstFilter2710NT

[InstFilter2710NT]
HKR,,"UpperFilters",0x00010000,"ScanUSBET"
HKR,,"LowerFilters",0x00010000,"FiltUSBET"


;---- I N T E R F A C E S ----

[USB2710.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2710.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2710.Interface

[USB2710.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2710.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2710.Interface

[USB2710.XP.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2710.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2710.Interface

[Capture2710.Interface]
AddReg = Capture.2710.AddReg


[Capture.2710.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"etVFW.dll"
HKR,,FriendlyName,,%USB2710.DeviceDesc%
HKLM,%Twain.Key%,"DSName",0,%USB2710.DeviceDesc%

; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}


;------ S E R V I C E S ------

[USB2710.NT.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2710
AddService = ScanUSBET,0x00000000,UpperInstall2710
AddService = FiltUSBET,0x00000000,LowerInstall2710

[USB2710.XP.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2710
AddService = ScanUSBET,0x00000000,UpperInstall2710
AddService = FiltUSBET,0x00000000,LowerInstall2710

[DriverInstall2710]
DisplayName   = %USB2710.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etDevice.sys

[UpperInstall2710]
DisplayName   = %USBscan.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etScan.sys

[LowerInstall2710]
DisplayName   = %etLower.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etFilter.sys



;---------------------  U S B 2 7 1 1  --------------------

[USB2711]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2711.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2711.XP]
Include       = ks.inf, kscaptur.inf, ksfilter.inf, sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT, STI.WIAVideo.Registration
AddReg        = CAP.AddReg, WIAUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyWIA, CAP.CopyEXE, CAP.CopyTwnXP
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 3
DeviceSubType = 1
Capabilities  = 0x11
Events        = STI.Events
DeviceData    = WIA.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"


;------------ H W ------------

[USB2711.HW]
AddReg = InstFilter2711

[InstFilter2711]
HKR,,UpperFilters,0,"etScan.sys"
HKR,,LowerFilters,0,"etFilter.sys"


[USB2711.NT.HW]
AddReg = InstFilter2711NT

[USB2711.XP.HW]
AddReg = InstFilter2711NT

[InstFilter2711NT]
HKR,,"UpperFilters",0x00010000,"ScanUSBET"
HKR,,"LowerFilters",0x00010000,"FiltUSBET"


;---- I N T E R F A C E S ----

[USB2711.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2711.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2711.Interface

[USB2711.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2711.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2711.Interface

[USB2711.XP.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2711.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2711.Interface


[Capture2711.Interface]
AddReg = Capture.2711.AddReg

[Capture.2711.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"etVFW.dll"
HKR,,FriendlyName,,%USB2711.DeviceDesc%
HKLM,%Twain.Key%,"DSName",0,%USB2711.DeviceDesc%

; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
    

;------ S E R V I C E S ------

[USB2711.NT.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2711
AddService = ScanUSBET,0x00000000,UpperInstall2711
AddService = FiltUSBET,0x00000000,LowerInstall2711

[USB2711.XP.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2711
AddService = ScanUSBET,0x00000000,UpperInstall2711
AddService = FiltUSBET,0x00000000,LowerInstall2711

[DriverInstall2711]
DisplayName   = %USB2711.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etDevice.sys

[UpperInstall2711]
DisplayName   = %USBscan.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etScan.sys

[LowerInstall2711]
DisplayName   = %etLower.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etFilter.sys



;---------------------  U S B 2 7 5 0  --------------------

[USB2750]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2750.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2750.XP]
Include       = ks.inf, kscaptur.inf, ksfilter.inf, sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT, STI.WIAVideo.Registration
AddReg        = CAP.AddReg, WIAUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyWIA, CAP.CopyEXE, CAP.CopyTwnXP
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 3
DeviceSubType = 1
Capabilities  = 0x11
Events        = STI.Events
DeviceData    = WIA.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"


;------------ H W ------------

[USB2750.HW]
AddReg = InstFilter2750

[InstFilter2750]
HKR,,UpperFilters,0,"etScan.sys"
HKR,,LowerFilters,0,"etFilter.sys"


[USB2750.NT.HW]
AddReg = InstFilter2750NT

[USB2750.XP.HW]
AddReg = InstFilter2750NT

[InstFilter2750NT]
HKR,,"UpperFilters",0x00010000,"ScanUSBET"
HKR,,"LowerFilters",0x00010000,"FiltUSBET"


;---- I N T E R F A C E S ----

[USB2750.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2750.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2750.Interface

[USB2750.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2750.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2750.Interface

[USB2750.XP.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2750.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2750.Interface

[Capture2750.Interface]
AddReg = Capture.2750.AddReg


[Capture.2750.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"etVFW.dll"
HKR,,FriendlyName,,%USB2750.DeviceDesc%
HKLM,%Twain.Key%,"DSName",0,%USB2750.DeviceDesc%

; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
    

;------ S E R V I C E S ------

[USB2750.NT.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2750
AddService = ScanUSBET,0x00000000,UpperInstall2750
AddService = FiltUSBET,0x00000000,LowerInstall2750

[USB2750.XP.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2750
AddService = ScanUSBET,0x00000000,UpperInstall2750
AddService = FiltUSBET,0x00000000,LowerInstall2750

[DriverInstall2750]
DisplayName   = %USB2750.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etDevice.sys

[UpperInstall2750]
DisplayName   = %USBscan.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etScan.sys

[LowerInstall2750]
DisplayName   = %etLower.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etFilter.sys



;---------------------  U S B 2 7 5 1  --------------------

[USB2751]
Include       = ks.inf, kscaptur.inf, ksfilter.inf
Needs         = KS.Registration, KSCAPTUR.Registration
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2751.NT]
Include       = ks.inf, kscaptur.inf, ksfilter.inf sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT
AddReg        = CAP.AddReg, STIUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopySTI, CAP.CopyEXE, CAP.CopyTwain
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 2
DeviceSubType = 0
Capabilities  = 1
Events        = STI.Events
ICMProfiles   = "sRGB Color Space Profile.icm"


[USB2751.XP]
Include       = ks.inf, kscaptur.inf, ksfilter.inf, sti.inf
Needs         = KS.Registration, KSCAPTUR.Registration.NT, STI.WIAVideo.Registration
AddReg        = CAP.AddReg, WIAUSD.AddReg, OEM.AddReg, OEM.Defaults.AddReg
CopyFiles     = CAP.CopySYS, CAP.CopyDLL, CAP.CopyWIA, CAP.CopyEXE, CAP.CopyTwnXP
UpdateInis    = CAP.UpdateIni

SubClass      = StillImage
DeviceType    = 3
DeviceSubType = 1
Capabilities  = 0x11
Events        = STI.Events
DeviceData    = WIA.DeviceData
ICMProfiles   = "sRGB Color Space Profile.icm"


;------------ H W ------------

[USB2751.HW]
AddReg = InstFilter2751

[InstFilter2751]
HKR,,UpperFilters,0,"etScan.sys"
HKR,,LowerFilters,0,"etFilter.sys"


[USB2751.NT.HW]
AddReg = InstFilter2751NT

[USB2751.XP.HW]
AddReg = InstFilter2751NT

[InstFilter2751NT]
HKR,,"UpperFilters",0x00010000,"ScanUSBET"
HKR,,"LowerFilters",0x00010000,"FiltUSBET"


;---- I N T E R F A C E S ----

[USB2751.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2751.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2751.Interface

[USB2751.NT.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2751.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2751.Interface

[USB2751.XP.Interfaces]
AddInterface = %KSCATEGORY_VIDEO%,  GLOBAL,Capture2751.Interface
AddInterface = %KSCATEGORY_CAPTURE%,GLOBAL,Capture2751.Interface


[Capture2751.Interface]
AddReg = Capture.2751.AddReg

[Capture.2751.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,ExtensionDLL,,"etVFW.dll"
HKR,,FriendlyName,,%USB2751.DeviceDesc%
HKLM,%Twain.Key%,"DSName",0,%USB2751.DeviceDesc%

; IAMVideoCompression installed as static interface on both output pins
HKR,PinFactory\0\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
HKR,PinFactory\1\Interfaces\{C6E13343-30AC-11d0-A18C-00A0C9118956},,,{C6E13343-30AC-11d0-A18C-00A0C9118956}
    

;------ S E R V I C E S ------

[USB2751.NT.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2751
AddService = ScanUSBET,0x00000000,UpperInstall2751
AddService = FiltUSBET,0x00000000,LowerInstall2751

[USB2751.XP.Services]
AddService = DCamUSBET,0x00000002,DriverInstall2751
AddService = ScanUSBET,0x00000000,UpperInstall2751
AddService = FiltUSBET,0x00000000,LowerInstall2751


[DriverInstall2751]
DisplayName   = %USB2751.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etDevice.sys

[UpperInstall2751]
DisplayName   = %USBscan.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etScan.sys

[LowerInstall2751]
DisplayName   = %etLower.DeviceDesc%
ServiceType   = 1		;SERVICE_KERNEL_DRIVER
StartType     = 3		;SERVICE_DEMAND_START
ErrorControl  = 1		;SERVICE_ERROR_NORMAL
ServiceBinary = %12%\etFilter.sys




;---------------------  C O M M O N  ----------------------

[CAP.AddReg]
HKR,,HardwareConfig,1,1
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,etDevice.sys
HKR,,OkToHibernate,3,1
HKR,,DontSuspendIfStreamsAreRunning,3,1 
HKR,,PageOutWhenUnopened,3,0
HKR,,PowerDownWhenUnopened,3,0

; ICustomCameraProp
HKCR,CLSID\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA},,,%CustomPlugIn%
HKCR,CLSID\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA}\InprocServer32,,,etProp.ax
HKCR,CLSID\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA}\InprocServer32,ThreadingModel,,Both
; This IID is aggregated for the filter given the CLSID of the property set
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA},,,%CustomPlugIn%
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA},IID,1, FB, 8E, 54, 85, C8, 86, 57, 4e, 0xb2, 0xfa, 0x80, 0x2b, 0x1b, 0x86, 0xc2, 0xaa

; CustomCamera Property Page
HKCR,CLSID\{3607A27C-2A4E-4437-A8D5-D273689A04BC},,,%CustomPropPage%
HKCR,CLSID\{3607A27C-2A4E-4437-A8D5-D273689A04BC}\InprocServer32,,,etProp.ax
HKCR,CLSID\{3607A27C-2A4E-4437-A8D5-D273689A04BC}\InprocServer32,ThreadingModel,,Both

; Associate property set with property page
HKLM,System\CurrentControlSet\Control\MediaSets\{85548EFB-86C8-4e57-B2FA-802B1B86C2AA}\PropertyPages\{3607A27C-2A4E-4437-A8D5-D273689A04BC},,,%CustomPropPage%

[STIUSD.AddReg]
; Still Image
HKR,,USDClass,,"{4C6E477B-E43B-4826-A4F4-C1D0CD73116A}"
HKCR,CLSID\{4C6E477B-E43B-4826-A4F4-C1D0CD73116A} ,,,%StillUSD%
HKCR,CLSID\{4C6E477B-E43B-4826-A4F4-C1D0CD73116A}\InProcServer32,,,%11%\etUSD.dll
HKCR,CLSID\{4C6E477B-E43B-4826-A4F4-C1D0CD73116A}\InProcServer32,ThreadingModel,,"Both"

[WIAUSD.AddReg]
HKR,,HardwareConfig,1,4
;
; The GUID in the following entries must match the class ID
; of the WIA minidriver (see wiacam.cpp).
;
;HKR,,USDClass,,"{8E3F2BAE-C8FF-4eff-AABD-0C58695389E8}"


[CAP.Sensor.AddReg]
; Register ePCCAP as a push-model application
;HKLM,%STIRegistration%,%StillAPP%,,"%10%\ePCCAP.exe /StiDevice:%%1 /StiEvent:%%2"

[CAP.SensorWIA.AddReg]
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Run","etMonitor",,"%10%\etMon.exe"
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce","etRun",,"%10%\etRun.exe -start"


[WIA.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={4DB1AD10-3391-11D2-9A33-00C04FA36145}

[CAP.CopyDLL]
etVFW.dll
emYUV.dll
etProp.ax

[CAP.CopySYS]
etDevice.sys
etScan.sys
etFilter.sys

[CAP.CopyTwain]
etTwain.ds

[CAP.CopyTwnXP]
etTwnXP.ds

[CAP.CopySTI]
etUSD.dll

[CAP.CopyWIA]
etMon.exe
etRun.exe

[CAP.CopyEXE]

[CAP.UpdateIni]
system.ini,drivers32,,"VIDC.I420=emYUV.dll"
system.ini,drivers32,,"VIDC.YUY2=emYUV.dll"

[STI.Events]
NewPicture = "%NewPicture%",{7EFBBC99-F7B8-4332-A983-378111C32966},"%StillAPP%"
SnapButton = "%SnapButton%",{A1039393-DF3A-476C-8F16-CE9ECC503E00},"%PreviewAPP%"



;-------------------------  O E M  ------------------------

; For hardware designs without EEPROM:  All OEM configuration data 
; in this section are active.
;
; For hardware designs with EEPROM:  FixupOWC, Optimization and OemID
; are specified in this section. All other configration data in this 
; section will have no effects and should be spedified in EEPROM.
;
; OemID is the vendor ID from EEPROM, but can be overridden here.
;
[OEM.AddReg]
HKR,settings\OEMSettings,Optimization,0x00010001,1          ; 1=ISO, 2=Bulk
HKR,settings\OEMSettings,FixUpOWC,0x00010001,12
HKR,settings\OEMSettings,FixUpATI,0x00010001,0              ; 1=enabled for multiple root hubs    
HKR,settings\OEMSettings,EnablePAL640x576,0x00010001,0      ; For 2820/2840
;;;HKR,settings\OEMSettings,BufferCount,0x00010001,8
;;;HKR,settings\OEMSettings,StrictHeader,0x00010001,0
;;;HKR,settings\OEMSettings,OemID,0x00010001,0
;;;HKR,settings\OEMSettings,PowerControl,0x00010001,0

; Board Configurations
HKR,settings\OEMSettings,Composite,0x00010001,1             ; Composite Input
HKR,settings\OEMSettings,SVideo,0x00010001,1                ; S-Video Input
HKR,settings\OEMSettings,SonyOnBoard,0x00010001,0           ; Sony Modules    
HKR,settings\OEMSettings,XceiveMTS,0x00010001,0             ; XC3028 Baseband Audio

; Driver Configurations
HKR,settings\OEMSettings,StrictI2cAccess,0x00010001,0       ; 0=Normal, 1=Strict
HKR,settings\OEMSettings,VideoSwitchMode,0x00010001,1       ; 0=Freeze, 1=Blackout
HKR,settings\OEMSettings,EnableSquarePixel,0x00010001,1     ; 1=enabled
HKR,settings\OEMSettings,Enable704,0x00010001,0             ; 1=enabled
HKR,settings\OEMSettings,EnableUSB1CMOS640,0x00010001,1     ; 1=enabled
HKR,settings\OEMSettings,DSFineTune,0x00010001,1            ; 1=enabled
HKR,settings\OEMSettings,GPIObyAP,0x00010001,0              ;
HKR,settings\OEMSettings,TVTuneByAP,0x00010001,0            ;
HKR,settings\OEMSettings,PowerOffIfIdle,0x00010001,0        ; for TV tuner

; OEM Devices Accessed from Applications Directly.
HKR,settings\OEMSettings,Oem0I2C,0x00010001,0x60
HKR,settings\OEMSettings,Oem0Type,0x00010001,2
HKR,settings\OEMSettings,Oem1I2C,0x00010001,0x60
HKR,settings\OEMSettings,Oem1Type,0x00010001,2
HKR,settings\OEMSettings,Oem2I2C,0x00010001,0x60
HKR,settings\OEMSettings,Oem2Type,0x00010001,2
HKR,settings\OEMSettings,Oem3I2C,0x00010001,0x60
HKR,settings\OEMSettings,Oem3Type,0x00010001,2

HKR,settings\OEMSettings,UVFactor,0x00000000,1.14159

; Tuner CFG & Overrides
;;;HKR,settings\OEMSettings,TunerIDBase,0x00010001,0
;;;HKR,settings\OEMSettings,TunerID7,0x00010001,21          ;CFG7 = SAM9082

; USB/Ext Audio Mux - 2820/2840 Only
;;;HKR,settings\OEMSettings,USBAudioMux,0x00010001,1
;;;HKR,settings\OEMSettings,ExtAudioMux,0x00010001,2

; The following OEM settings are obsolete. Please set default
; ProcAmp values in section [OEM.Defaults.AddReg] below.
;
;;;HKR,settings\OEMSettings,DefaultProcAmp,0x00010001,0x80204020
;;;HKR,settings\OEMSettings,DefaultSharpness,0x00010001,2
;;;HKR,settings\OEMSettings,DefaultGamma,0x00010001,32

; DTV Country Code - 2880 Only
;
; Option 1 - Comment out the following line and use the driver default.
;
;            Default DTVCountry =  1 (USA)     if ATSC demod is on board.
;            Default DTVCountry = 49 (Germany) if DVBT demod is on board.
;
;            Driver will convert channel number to center frequency,
;            using a table corresponding to DirectShow country code.
;
; Option 2 - Set DTVCountry to target country code, e.g., 86(China) or 
;            886(Taiwan), if option 1 above does not work. Driver will 
;            convert channel number to center frequency, using a table
;            corresponding to DTVCountry.
;
; Option 3 - Set DTVCountry to 0 if application is capable of providing
;            the DTV frequencies to driver.
;
;;;HKR,settings\OEMSettings,DTVCountry,0x00010001,0	    


; OEM Property Defaults:
;
; This section provides property defaults for the WDM driver.
;
; If EEPROM is on board, some of these property defaults are provided
; by EEPROM. The remaining perperty defaults are specified here.
;
; A property default is only meaningful if the corresponding property
; is not yet defined in the system registry.
;
[OEM.Defaults.AddReg]
HKR,settings\PropDefaults,Brightness,0x00010001,110         ;
HKR,settings\PropDefaults,Contrast,0x00010001,32            ;
HKR,settings\PropDefaults,Hue,0x00010001,64                 ;
HKR,settings\PropDefaults,Saturation,0x00010001,32          ;
HKR,settings\PropDefaults,Sharpness,0x00010001,4            ;
HKR,settings\PropDefaults,Gamma,0x00010001,32               ;

HKR,settings\PropDefaults,Mirror,0x00010001,0               ; 0=OFF, 1=ON
HKR,settings\PropDefaults,Flip,0x00010001,0                 ; 0=OFF, 1=ON
HKR,settings\PropDefaults,AutoExposure,0x00010001,0         ; 0=OFF, 1=ON
HKR,settings\PropDefaults,AEMode,0x00010001,0               ; 0=Dark, 1=Normal
HKR,settings\PropDefaults,AE_Level,0x00010001,3             ; Target AE (0-6)        
HKR,settings\PropDefaults,Exposure,0x00010001,18            ;
HKR,settings\PropDefaults,LightTemperature,0x00010001,0     ;
HKR,settings\PropDefaults,LightFreq,0x00010001,1            ; 0=60Hz, 1=50Hz
HKR,settings\PropDefaults,AutoWhiteBalance,0x00010001,1     ; 0=OFF , 1=ON
HKR,settings\PropDefaults,AWB_R,0x00010001,46               ;
HKR,settings\PropDefaults,AWB_B,0x00010001,56               ;
HKR,settings\PropDefaults,WindowSize,0x00010001,0           ; 0=640x480, 1=320x240, 2=1280x960
HKR,settings\PropDefaults,MonitorType,0x00010001,1          ; 0=CRT,  1=LCD
HKR,settings\PropDefaults,Volume,0x00010001,8               ; 

HKR,settings\PropDefaults,VideoStandard,0x00010001,1        ; 1=NTSC, 0x10=PAL_B, 0x40000=SECAM_L
HKR,settings\PropDefaults,Deinterlace,0x00010001,1          ; 1=Weave, 2=Bob
HKR,settings\PropDefaults,VCRMask,0x00010001,0              ; # of lines masked out
HKR,settings\PropDefaults,MaskColor,0x00010001,1            ; 0=Gray, 1=Black

HKR,settings\OEMSettings,Use_CMOS_Scaler,0x00010001,0           ; for real SXGA Use CMOS scaler. 1 = CMOS scaler
HKR,settings\OEMSettings,Use_Lens_Correction,0x00010001,0x01    ; for Lens Correction setting. 
								; 0 = don't use about lens settion , 0x01 = Largan lens  
HKR,settings\OEMSettings,Use_Dark_Higher_fps,0x00010001,1       ; 1 = for dark mode use higher fps 
HKR,settings\OEMSettings,Use_Color_Matrix,0x00010001,2          ; 1 = enable Color Matrix 100%
								; 2 = Color Matrix 75%
								
HKR,settings\OEMSettings,HYN_RG_BG_Ratio,0x00010001,0x847A      ; for HYN7131E
HKR,settings\OEMSettings,HYN7131R_RG_BG_Ratio,0x00010001,0x847A ; for HYN7131R
HKR,settings\OEMSettings,HYN7141B_RG_BG_Ratio,0x00010001,0x847A ; for HYN7141B
HKR,settings\OEMSettings,MIC0360_RG_BG_Ratio,0x00010001,0x847A  ; for MIC0360
HKR,settings\OEMSettings,MIC1300_RG_BG_Ratio,0x00010001,0x847A  ; for MIC1300
HKR,settings\OEMSettings,CIS_V15_RG_BG_Ratio,0x00010001,0x8080  ; for CIS_V15
HKR,settings\OEMSettings,CIS_V10_RG_BG_Ratio,0x00010001,0x8080  ; for CIS_V10
HKR,settings\OEMSettings,ICM_108W_RG_BG_Ratio,0x00010001,0x8080 ; for ICM_108W
HKR,settings\OEMSettings,ICM_105C_RG_BG_Ratio,0x00010001,0x8080 ; for ICM_105C
HKR,settings\OEMSettings,TASC_5130D_RG_BG_Ratio,0x00010001,0x8080 ; for TASC5130D


HKR,settings\OEMSettings,DISABLE_I420_176x144,0x00010001,0  ; 1 = Disable I420  176 x 144
HKR,settings\OEMSettings,DISABLE_I420_352x288,0x00010001,0  ; 1 = Disable I420  352 x 288
HKR,settings\OEMSettings,DISABLE_I420_800x600,0x00010001,1  ; 1 = Disable I420  800 x 600

HKR,settings\OEMSettings,DISABLE_YUY2_176x144,0x00010001,0  ; 1 = Disable YUY2  176 x 144
HKR,settings\OEMSettings,DISABLE_YUY2_352x288,0x00010001,0  ; 1 = Disable YUY2  352 x 288
HKR,settings\OEMSettings,DISABLE_YUY2_800x600,0x00010001,1  ; 1 = Disable YUY2  800 x 600
HKR,settings\OEMSettings,DISABLE_YUY2_1024x768,0x00010001,1 ; 1 = Disable YUY2 1024 x 768
HKR,settings\OEMSettings,DISABLE_YUY2_1280x800,0x00010001,1 ; 1 = Disable YUY2 1280 x 800
HKR,settings\OEMSettings,DISABLE_YUY2_1280x960,0x00010001,0 ; 1 = Disable YUY2 1280 x 960
HKR,settings\OEMSettings,DISABLE_YUY2_1280x1024,0x00010001,0 ; 1 = Disable YUY2 1280 x 1024

HKR,settings\OEMSettings,Q1280,0x00010001,0                 ; CMOS 1280 (0 = 16 bit,1 = 8 bit)
HKR,settings\OEMSettings,EnableSelectiveSuspend,0x00010001,1; Selective Suspend
;;;HKR,settings\OEMSettings,For_OemID,0x00010001,1    	    ;1 = for Clevo
HKR,settings\OEMSettings,DefectPixel,0x00010001,1           ; Defect Pixel Compensation

;--------------------- S T R I N G S -----------------------

[Strings]
;---------------
;Non-Localizable
;---------------
KSCATEGORY_CAPTURE = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO   = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
ProxyVCap.CLSID    = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

Twain.Key          = "Software\USB2800\Camera"
CustomPlugIn       = "etProp Custom Interface"
CustomPropPage     = "etProp Custom Property Page"
StillUSD           = "ET USB Still Image USD"
STIRegistration    = "Software\Microsoft\Windows\CurrentVersion\StillImage\Registered Applications"
StillWIA           = "USB Still Image WIA"

;---------------
;Localizable
;---------------
Vendor             = "LWS"
DiskLabel          = "eMPIA Driver Disk"
NewPicture         = "ET New Picture Requested"
SnapButton         = "ET Snapshot Button Pressed"
StillAPP           = "ET2700 PC CAM Application"
PreviewAPP	       = "eMPIA AMCAP"
USBscan.DeviceDesc = "ET USB Still Image Capture Device"
etLower.DeviceDesc = "ET USB Device Lower Filter"


USB2710.DeviceDesc = "LWS-Camera-M"
USB2711.DeviceDesc = "LWS-Camera-M"
USB2750.DeviceDesc = "LWS-Camera-M"
USB2751.DeviceDesc = "LWS-Camera-M"