;------------------------------------------------------------------
;
;   ETAUDIO.INF -- This file contains installation information
;                  for eMPIA USB 2.0 Audio Devices:  EM2801,
;                  EM2711.
;
;       
;   This installation is for Windows 2000 and XP.
;
;   Copyright (C) LWS. 2004-2005 
;
;------------------------------------------------------------------

[Version]
Signature   = "$CHICAGO$"
Class       = MEDIA
ClassGUID   = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider    = %Vendor%
CatalogFile = emWHQL.cat
DriverVer   = 07/01/2005, 2.5.0701.0

[SourceDisksNames]
1 = %DiskLabel%,etAudio.sys,,

[SourceDisksFiles]
etAudio.sys = 1

[Manufacturer]
%Mfg%=Model

[Model]
;; %etAudio.DeviceDesc%=etAudio, USB\CLASS_01

%etAudio.DeviceDesc%=etAudio, USB\VID_EB1A&PID_2711&MI_01

[DestinationDirs]
etAudio.CopyList=10,system32\drivers

[etAudio]
AlsoInstall= ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles  = etAudio.CopyList
AddReg     = etAudio.AddReg

[etAudio.CopyList]
etAudio.sys

[etAudio.Interfaces]
AddInterface = %KSCATEGORY_AUDIO%,      %KSNAME_Wave%,          etAudio.I.Wave
AddInterface = %KSCATEGORY_RENDER%,     %KSNAME_Wave%,          etAudio.I.Wave
AddInterface = %KSCATEGORY_CAPTURE%,    %KSNAME_Wave%,          etAudio.I.Wave
AddInterface = %KSCATEGORY_AUDIO%,      %KSNAME_Topology%,      etAudio.I.Topo
AddInterface = %KSCATEGORY_RENDER%,     %KSNAME_Topology%,      etAudio.I.Topo
AddInterface = %KSCATEGORY_CAPTURE%,    %KSNAME_Topology%,      etAudio.I.Topo


[etAudio.AddReg]
HKR,,AssociatedFilters,,"wdmaud"
HKR,,Driver,,etAudio.sys
HKR,,NTMPDriver,,"etAudio.sys"
;; HKR,,NTMPDriver,,"etAudio.sys,sbemul.sys"
HKR,Drivers,SubClasses,,"wave, mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%etAudio.DeviceDesc%
HKR,Drivers\mixer\wdmaud.drv,Description,,%etAudio.DeviceDesc%
HKLM,%MediaCategories%\%etAudio.NameGuid%,Name,,%etAudio.Name%
HKLM,%Audio.Key%,"DeviceName",0,%etAudio.DeviceDesc%


[etAudio.I.Wave]
AddReg=etAudio.I.Wave.AddReg

[etAudio.I.Wave.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%etAudio.Wave.szPname%

[etAudio.I.Topo]
AddReg=etAudio.I.Topo.AddReg

[etAudio.I.Topo.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%etAudio.Topo.szPname%


[etAudio.NTX86]
Include=ks.inf,wdmaudio.inf
Needs=KS.Registration, WDMAUDIO.Registration
CopyFiles = etAudio.CopyList
AddReg    = etAudio.AddReg


[etAudio.NTX86.Interfaces]
AddInterface    = %KSCATEGORY_AUDIO%,   %KSNAME_Wave%,          etAudio.I.Wave
AddInterface    = %KSCATEGORY_RENDER%,  %KSNAME_Wave%,          etAudio.I.Wave
AddInterface    = %KSCATEGORY_CAPTURE%, %KSNAME_Wave%,          etAudio.I.Wave
AddInterface    = %KSCATEGORY_AUDIO%,   %KSNAME_Topology%,      etAudio.I.Topo


[etAudio.NTX86.Services]
include         = wdmaudio.inf
needs           = wdmaudio.registration.services
AddService      = etAudio, 0x00000002, etAudio_Service_Inst


[etAudio_Service_Inst]
DisplayName     = %etAudio.DeviceDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %10%\system32\drivers\etAudio.sys


[Strings]
;---------------
;Non-Localizable
;---------------
KSNAME_Wave          = "ET Wave"
KSNAME_Topology      = "ET Topology"
Proxy.CLSID          = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO     = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER    = "{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE   = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
etAudio.NameGuid     = "{855DA333-EB5D-4910-82E7-18B49EF2671C}"
MediaCategories      = "SYSTEM\CurrentControlSet\Control\MediaCategories"
Audio.Key            = "Software\USB2800\CameraAudio"

;---------------
;Localizable
;---------------
Vendor               = "LWS"
DiskLabel            = "eMPIA EM28xx Driver Disk"
Mfg                  = "eMPIA Technology - Audio"
etAudio.DeviceDesc   = "ET USB EMP Audio Device"
etAudio.Topo.szPname = "ET USB EMP Audio Topology"
etAudio.Wave.szPname = "ET USB EMP Audio Device"
etAudio_MIDI         = "ET USB EMP MIDI Device"
etAudio.Name         = "ET USB EMP Audio Device"

